Vanessa Ulloa

Daniel Kushner

CST 311

26 May 2015

Lab 4

1. 4 fields:
   1. Source Port
   2. Destination Port
   3. Length
   4. Checksum
2. 2 bytes
3. Length: 58
4. 65535 bytes
5. 65535
6. Protocol: UDP (17)
7. The 1st packet has a Source Port of 4334, the 2nd packet has a Destination port of 161. The 2nd packet has a Source Port if 161 and a Destination Port of 4334. The same with the Internet Protocol Source IP addresses.